{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["询价报价表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"询价报价表","index":0,"n_rows":52,"n_cols":10,"rows_kept":52,"merged":[[0,0,0,1],[1,0,1,9],[2,1,2,2],[2,3,2,4],[3,1,4,2],[3,3,3,4],[3,8,15,8],[4,3,4,4],[5,1,5,2],[5,3,5,4],[6,1,6,2],[6,3,6,4],[7,1,7,2],[7,3,7,4],[8,1,8,2],[8,3,8,4],[9,1,9,2],[9,3,9,4],[10,1,10,2],[10,3,10,4],[11,1,11,2],[11,3,11,4],[12,1,12,2],[12,3,12,4],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[15,3,15,4],[16,1,18,2],[16,3,16,4],[16,8,30,8],[17,3,17,4],[18,3,18,4],[19,1,21,2],[19,3,19,4],[20,3,20,4],[21,3,21,4],[22,1,22,2],[22,3,22,4],[23,1,23,2],[23,3,23,4],[24,1,24,2],[24,3,24,4],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[27,3,27,4],[28,1,28,2],[28,3,28,4],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[31,9,38,9],[32,1,32,2],[32,3,32,4],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,1,35,2],[35,3,35,4],[36,1,36,2],[36,3,36,4],[37,1,37,2],[37,3,37,4],[38,1,38,2],[38,3,38,4],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,1,41,2],[41,3,41,4],[42,1,42,2],[42,3,42,4],[43,1,43,2],[43,3,43,4],[44,1,44,2],[44,3,44,4],[45,1,45,2],[45,3,45,4],[46,1,46,2],[46,3,46,4],[47,1,47,2],[47,3,47,4],[48,1,48,2],[48,3,48,4],[49,1,49,2],[49,3,49,4],[50,1,50,2],[50,3,50,4],[51,1,51,2],[51,3,51,4]],"flags":["formulas_cached_only"]}
["附件"]
["惠州新材料产业园起步区1号公共应急池及一期配套管网建设项目钢管及管件、阀门采购项目询价报价表"]
["序号","材料名称",null,"规格型号",null,"单位","数量","报价（元）","防腐要求","备注"]
[1,"螺旋缝埋弧焊钢管(Q345B)",null,"D219*6",null,"米",1,null,"1、喷射除锈:喷石英砂,管道外壁除锈等级Sa2.5。\n2、管道内壁涂敷无溶剂液体环氧涂料，干膜厚度应≥200μm。\n3、架空管道外防腐:环氧富锌底漆1层（干膜厚度≥50μm）、环氧云铁中间漆1层（干膜厚度≥50μm）、丙烯酸面漆2层（干膜厚度≥40μm）。\n4、埋地管道内防腐：一层底渗加两层PE胶带(特加强级)。"]
[2,null,null," D610*10",null,"米",1]
[3,"无缝钢管(Q345B)",null,"D34*4",null,"米",1]
[4,"90°热煨弯管(Q345B)",null,"管外径×壁厚 \n630×10mm以内",null,"个",1]
[5,"55°热煨弯管(Q345B)",null,"管外径×壁厚 \n630×10mm以内",null,"个",1]
[6,"45°热煨弯管(Q345B)",null,"管外径×壁厚 \n630×10mm以内",null,"个",1]
[7,"15°热煨弯管(Q345B)",null,"管外径×壁厚 \n630×10mm以内",null,"个",1]
[8,"45°热煨弯管(Q345B)",null,"管外径×壁厚 \n219*8mm以内",null,"个",1]
[9,"90°热煨弯管(Q345B)",null,"管外径×壁厚\n 219*8mm以内",null,"个",1]
[10,"12°冷煨弯管(Q345B)",null,"管外径×壁厚 \n630×10mm以内",null,"个",1]
[11,"三通(直缝埋弧焊钢管)Q345B",null,"DN600*200",null,"个",1]
[12,"三通(直缝埋弧焊钢管)Q345B",null,"DN600",null,"个",1]
[13,"偏心变径管Q345B",null,"DN600*200",null,"个",1]
[14,"螺旋缝埋弧焊钢管(Q345B)",null," D600*15",null,"米",1,null,"1、前处理：喷砂除锈达Sa 2.5级或电动砂轮除锈达到St级标准，清理掉表面的灰尘、砂粒,使表面清洁、干燥。\n2、钢管内防腐：钢管内防腐: 在钢管内壁先涂底漆三遍,采用KY-2021厚浆型环氧重防腐涂料(铁红色),厚约80umx3。面漆两遍,采用KY-2026高抗水性环氧重防腐涂料(棕黑色),厚约80umx2,涂层干膜厚约400um。\n3、埋地钢管外防腐:在钢管外壁先涂底漆三遍,采用KY-2021厚浆型环氧重防腐涂料(铁红色),厚约80umx3。钢管外壁加设玻璃纤维布(无碱、无腊)二层。面漆三遍,采用KY-2026高抗水性环氧重防腐涂料(棕黑色),厚约80umx3,涂层干膜厚约500um。\n4、外露、架空钢管外壁防腐:在钢管外壁先涂底漆三遍,采用KY-2021厚浆型环氧重防腐涂料(铁红色),厚约80umx3。面漆两遍,采用KY-2062脂肪族聚氨脂防腐耐晒面漆(中灰或天蓝色),厚约35umx2;涂层干膜厚310um。"," "]
[15,null,null," D200*14",null,"米",1]
[16,null,null," D100*8",null,"米",1]
[17,"焊接钢管(Q345B)",null,"DN65",null,"米",1]
[18,null,null,"DN50",null,"米",1]
[19,null,null,"DN20",null,"米",1]
[20,"90°弯头(Q345B)",null,"DN600",null,"个",1]
[21,"90°弯头(Q345B)",null,"DN200",null,"个",1]
[22,"90°弯头(Q345B)",null,"DN100",null,"个",1]
[23,"90°弯头(Q345B)",null,"DN50",null,"个",1]
[24,"三通/支管台(Q345B)",null,"DN600×DN600",null,"个",1]
[25,"三通/支管台(Q345B)",null,"DN600×DN200",null,"个",1]
[26,"三通/支管台(Q345B)",null,"DN200×DN100",null,"个",1]
[27,"三通/支管台(Q345B)",null,"DN200×DN200",null,"个",1]
[28,"三通(Q345B)",null,"DN200×DN65",null,"个",1]
[29,"暗杆闸阀",null,"DN100 PN16 Z45F-16Q",null,"个",1,null,null,"配法兰、垫片及紧固件"]
[30,"暗杆闸阀",null,"DN20 PN16 Z25F-16H",null,"个",1]
[31,"电传动法兰式蝶阀",null,"DN600，PN16 D941F-16Q ",null,"个",1]
[32,"电传动法兰式蝶阀",null,"DN200，PN16 D941F-16Q",null,"个",1]
[33,"电传动法兰式蝶阀",null,"DN100，PN16 D941F-16Q",null,"个",1]
[34,"电传动法兰式蝶阀",null,"DN65，PN16 D941F-16Q",null,"个",1]
[35,"电传动法兰式蝶阀",null,"DN50，PN16 D941F-16Q",null,"个",1]
[36,"止回阀",null,"DN100，PN16 H44F-16Q",null,"个",1]
[37,"阀门（球墨铸铁）",null,"D25，Z41F-10C闸阀，1.0Mpa",null,"个",1]
[38,"阀门（球墨铸铁）",null,"DN200，Z41F-10C闸阀，1.1Mpa",null,"个",1]
[39,"阀门（球墨铸铁）",null,"DN600，Z41F-10C闸阀，1.2Mpa",null,"个",1]
[40,"带颈平焊法兰",null,"SO600-16",null,"个",1]
[41,"带颈平焊法兰",null,"SO200-16",null,"个",1]
[42,"带颈平焊法兰",null,"SO100-16",null,"个",1]
[43,"带颈平焊法兰",null,"SO65-16",null,"个",1]
[44,"带颈平焊法兰",null,"SO50-16",null,"个",1]
[45,"聚四氟乙烯垫片",null,"600-16",null,"个",1]
[46,"聚四氟乙烯垫片",null,"200-16",null,"个",1]
[47,"聚四氟乙烯垫片",null,"100-16",null,"个",1]
[48,"聚四氟乙烯垫片",null,"65-16",null,"个",1]
[49,"聚四氟乙烯垫片",null,"50-16",null,"个",1]