{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"merged":[[0,0,0,8],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,2,8],[3,1,13,1],[4,7,5,7],[14,0,14,8],[16,0,16,8],[17,0,17,8],[18,0,18,5],[19,0,19,5],[19,6,19,7]],"flags":["formulas_cached_only"]}
["惠州新材料产业园配套区基础设施建设项目横二路（一号标）施工图设计、施工总承包（EPC）钢筋混凝土管采购项目询价报价表"]
["序号","材料名称","规格型号","技术参数","单位","数量","报价（元）","防腐要求","备注"]
[]
[1,"Ⅱ级钢筋混凝土管排水管","DN300","承插口","m",1,null,null,"含胶圈"]
[2,null,"DN400","承插口","m",1,null,"内壁防腐，采用聚氨酯防腐涂料，防腐总干膜厚度不小于240＋20um。具体实施按《建筑防腐蚀工程施工质量验收标准》GB/T50224-2018相关要求执行。","含胶圈"]
[3,null,"DN500","承插口","m",1,null,null,"含胶圈"]
[4,null,"DN600","承插口","m",1,null,null,"含胶圈"]
[5,null,"DN800","承插口","m",1,null,null,"含胶圈"]
[6,null,"DN1000","承插口","m",1,null,null,"含胶圈"]
[7,null,"DN1200","承插口","m",1,null,null,"含胶圈"]
[8,null,"DN1350","企口管","m",1,null,null,"含胶圈"]
[9,null,"DN1500","企口管","m",1,null,null,"含胶圈"]
[10,null,"DN1650","企口管","m",1,null,null,"含胶圈"]
[11,null,"DN1800","企口管","m",1,null,null,"含胶圈"]
["注：单价包含货物制造费、运输费、装卸费、税金（注明税率）、售后服务等交付采购人使用前所有可能发生的费用；数量以采购人实际采购数量为准，送货量月结80%，当年结算至97%，质量保证金3%完工一年后付清，具体以签订的合同条款为准。"]
[]
["供应商名称："]
["供应商地址："]
["联系人："]
["联系电话：",{"$nulls":5},"日期：2023年   月    日"]